**Led controller**

|  |  |
| --- | --- |
| Author | Cas Truyers |

Content

[Introduction 3](#_Toc73307918)

[Materials and methods 4](#_Toc73307919)

[2.1 Materials 4](#_Toc73307920)

[2.1.1 Hardware 4](#_Toc73307921)

[2.1.2 Software 4](#_Toc73307922)

[2.1.3 Bill of materials 5](#_Toc73307923)

[2.2 Methods 7](#_Toc73307924)

[2.2.1 Research 7](#_Toc73307925)

[2.2.2 Supplier 7](#_Toc73307926)

[2.2.3 Altium schematic design 7](#_Toc73307927)

[2.2.4 Altium PCB design 7](#_Toc73307928)

[Results 8](#_Toc73307929)

[3.1 LED drivers 8](#_Toc73307930)

[3.1.1 Operation 8](#_Toc73307931)

[3.1.2 Schematic 8](#_Toc73307932)

[3.1.3 PCB design 9](#_Toc73307933)

[3.1.4 Mechanical design 9](#_Toc73307934)

[3.1.5 Finalized product 9](#_Toc73307935)

[3.2 Voltage regulator 10](#_Toc73307936)

[3.2.1 Operation 10](#_Toc73307937)

[3.2.2 Schematic 10](#_Toc73307938)

[3.2.3 PCB design 10](#_Toc73307939)

[3.2.4 Mechanical design 11](#_Toc73307940)

[3.2.5 Finalized product 11](#_Toc73307941)

[3.3 ESP32 12](#_Toc73307942)

[3.3.1 Operation 12](#_Toc73307943)

[3.3.2 Schematic 12](#_Toc73307944)

[3.3.3 PCB design 13](#_Toc73307945)

[3.3.4 Mechanical design 13](#_Toc73307946)

[3.3.5 Finalized product 13](#_Toc73307947)

[Discussion 14](#_Toc73307948)

[4.1 Difficulties 14](#_Toc73307949)

[4.1.1 LEDS 14](#_Toc73307950)

[4.1.2 Backorder 14](#_Toc73307951)

[4.1.3 Enabling LED driver 14](#_Toc73307952)

[4.2 Reflection 14](#_Toc73307953)

[4.2.1 PCB silkscreen 14](#_Toc73307954)

[4.2.2 Programming 14](#_Toc73307955)

[4.3 Conclusion 14](#_Toc73307956)

# Introduction

The emergence of indoor vertical agriculture with LEDs is stimulating new technological developments to operate the LEDs efficiently. The LED controller discussed in this application note is used in vertical farming for controlling and automating the LED infrastructure. The schematic used for the LED controller, is found in the Elektor magazine [1]. The design consists of several segments, each with different functions. With the LED drivers and the integrated ESP32 module, a solution is created to control the intensity and light cycles through a convenient web interface. Four different LED chains can be individually controlled with this model. Each chain can contain LEDs with a specific light spectrum. Combining the LED chains and controlling them individually, creates an optimal light spectrum for a specific plant and its growing stage. In this application note, the process of designing the PCB and associated research is described.

# Materials and methods

## Materials

### Hardware

The LED controller consists of about a hundred components, most of which are common such as resistors, capacitors, inductors and semiconductors. There are three different modules used in the design, the LM2576HVS, MagI³C-LDHM and the ESP-32-WROVER-B. [1]

The LM2576HVS is a step-down converter that converts an input between 4V and 60V to an adjustable constant voltage between 1.23V and 57V. This is determined by its arrangement. [2]

The MagI³C-LDHM is an LED driver module that provides an adjustable constant current. The current is determined by connecting a certain resistance value to its Iset pin. It needs a minimum of 4.5V and tolerates a maximum of 60V at its input. This module provides up to 450mA. [3] With this module, LEDs can be dimmed with the use of PWM signals.

ESP32-WROVER-B is a powerful, generic WiFi-BT-BLE MCU module that targets a wide variety of applications. [4] In this design, the ESP32-WROVER-B generates four PWM signals, 1 for each LED driver. The module is programmed to connect to the web and be controlled through a web interface.

A specific led must be chosen for a particular application. After research, the LUXEON Sunplus 35 LEDs are preferred for vertical farming applications, instead of the LED series from Würth Elektronik recommended by the Elektor magazine [1]. The LUXEON Sunplus 35 LEDs are suitable for vertical farming because they produce little heat. [5] Therefore they can be placed closer to the plant and thus save space, which is critical in vertical farming. The LEDs from Würth Elektronik emit more photons per electric usage and thus are more efficient. But they are meant to be placed in greenhouses at a long distance from the plant and thus produce more heat. Therefore they are not suitable for our application.

### Software

The Arduino IDE is used to program the ESP-32-WROVER-B. This requires the ESP32 library for Arduino to be installed. The Arduino IDE is preferred over other IDEs because the associated code is written for the Arduino IDE. [1]

To draw the schematics and design the PCBs, Altium designer is used. Altium Designer, compared to other software such as Aegle, has more features and is more often used in the professional field. Altium also offers many easy-to-reference instructions.

### Bill of materials

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Bill of materials** | | | | | |
| ***Description*** | ***Manufacturer*** | ***Qnt*** | **Price p/u** | **Digikey Part Number** | Est. Delivery Date |
| *Resistor* |  | *12* |  |  |  |
| 10 kΩ, thick film, 5%, 0.1W, 150V | Multicomp | 1 | €0.09 | 541-CRCW120610K0JNEBCT-ND | 6/04/2021 |
| 1 kΩ, thick film, 5%, 0.1W, 150V | Multicomp | 1 | €0.09 | 2019-RK73B2ATTD102JCT-ND | 6/04/2021 |
| 2.7 kΩ, thick film, 5%, 0.1W, 150V | Multicomp | 1 | €0.09 | P2.7KACT-ND | 6/04/2021 |
| 1.6 kΩ, thick film, 1%, 0.125W,150V | Multicomp | 1 | €0.09 | P1.60KCCT-ND | 6/04/2021 |
| *Inductor* |  | *6* |  |  |  |
| EMI suppression ferrite, 1500Ohm | Würth Elektronik | 1 | €0.19 | 732-4649-1-ND | 6/04/2021 |
| SMD common mode line filter 10uH | Würth Elektronik | 1 | €2.10 | 732-1476-1-ND | 6/04/2021 |
| SMD power inductor, 10uH, 800mA | Würth Elektronik | 1 | €0.84 | 732-11499-1-ND | 6/04/2021 |
| SMD power inductor 2.2uH, 2.5A | Würth Elektronik | 1 | €1.44 | 732-1250-1-ND | 6/04/2021 |
| Power Inductor (SMD), 470 µH, 600 mA | Würth Elektronik | 1 | €1.81 | 732-4039-1-ND | 6/04/2021 |
| Ferrite bead, 31 Ohm, 3A, size 1206 | Würth Elektronik | 1 | €0.20 | 732-1626-1-ND | 6/04/2021 |
| *Capacitor* |  | *8* |  |  |  |
| 4.7 µF, 100 V, 7.7 x 6.3mm | Würth Elektronik | 1 | €1.53 | 732-11980-1-ND | 6/04/2021 |
| 100 nF, 100 V, X7R, 0805 | Würth Elektronik | 1 | €0.09 | 732-12244-1-ND | 6/04/2021 |
| 27 µF, 100 V, 20%, 8mm, radial | Würth Elektronik | 1 | €0.36 | 732-9253-1-ND | 6/04/2021 |
| 47 µF, 10 V, 2312 | Vishay | 1 | €0.53 | 718-1087-1-ND | 6/04/2021 |
| 4.7 µf, 50V, X7R, 1210 | Murata Electronics | 1 | €0.49 | 490-1864-1-ND | 6/04/2021 |
| 100 µF, 10 V, 5.5 x 5.5mm | Würth Elektronik | 1 | €0.48 | 732-6410-1-ND | 6/04/2021 |
| 2.2 µF, 100V, X7R, 1210 | Kemet | 1 | €0.64 | 399-5511-1-ND | 6/04/2021 |
| 1 nF, 16V, X7R, 0603 | Würth Elektronik | 1 | €0.09 | 732-7953-1-ND | 6/04/2021 |
| *Semiconductor* |  | *9* |  |  |  |
| MBRS540, 40 V, 5 A, Vf=550 mV @ If=5 A | ON Semiconductor | 1 | €0.47 | MBRS540T3GOSCT-ND | 6/04/2021 |
| LED, green, 3 mm | Würth Elektronik | 1 | €0.21 | 732-5012-ND | 6/04/2021 |
| LED, red, 3 mm | Würth Elektronik | 1 | €0.21 | 732-5013-ND‎ | 6/04/2021 |
| LED, yellow, 3 mm | ürth Elektronik | 1 | €0.21 | 732-5014-ND | 6/04/2021 |
| LED, blue, 3 mm | Würth Elektronik | 1 | €0.21 | 732-5011-ND‎ | 6/04/2021 |
| BC847C, 45 V, 100 mA, 250 mW, hfe=400 | NXP | 1 | €0.10 | 1727-2924-1-ND | 6/04/2021 |
| MagI3C LED | Würth Elektronik | 1 | €6.67 | 732-6218-1-ND | 6/04/2021 |
| LM2576HVS-ADJ | Texas Instruments | 1 | €5.93 | LM2576HVS-ADJ/NOPB-ND | 6/04/2021 |
| ESP-32-WROVER-B | Espressif | 1 | €4.22 | 1904-1034-1-ND | 6/04/2021 |
| *Other* |  | *13* |  |  |  |
| Switch, tactile, 12 V, 50 mA, 6x6 mm | Würth Elektronik | 1 | €0.09 | ‎450-1650-ND | 6/04/2021 |
| Terminal block 5.08 mm, 2-way, 630 V | Würth Elektronik | 9 | €1.41 | 277-1273-ND | 6/04/2021 |
| header male 5 pin, 0.1" pitch vertical | Fisher Elektronik | 1 | €0.21 | 732-5318-ND | 6/04/2021 |
| header male 6 pin, 0.1" pitch vertical | Fisher Elektronik | 1 | €0.28 | 732-5319-ND | 6/04/2021 |
| header male 4 pin, 0.1" pitch vertical | Fisher Elektronik | 1 | €0.15 | 732-5317-ND | 6/04/2021 |
| Jumper, 1x2, vertical | TE Connectivity | 1 | €0.11 | 732-5315-ND | 6/04/2021 |
| 4 x Jumper, 2 way, 2.54 mm | FCI | 4 | €0.09 | S9341-ND | 6/04/2021 |

## Methods

### Research

#### Schematic design research

Schematic design research has been done by examining the schematic of the LED controller published by Elektor [1]. The complete schematic and all the components needed are found in this magazine.

#### Individual component research

All the individual components were examined according to their datasheets. In addition to the datasheet, research has been done on the MagI3C module through the given webinar from Würth Elektronik [6]. A video from Würth Elektronik demonstrating the module and giving a short explanation of its function was also examined [7].

### Supplier

#### Requirements

Because there are more than 100 components it is recommended to order the components from one supplier. This way an organized overview of the order is kept. Delivery time and delivery costs are also important to take into account.

#### DigiKey

Digikey has been chosen as a supplier because it meets these requirements. It has one of the largest assortments and has all the required components in stock.

### Altium schematic design

The next step is drawing the schematic in Altium designer. Elektor’s schematic is divided into three smaller schematics for each module and its associated components. This way the project is more manageable. The LED driver, ESP-32-WROVER-B and the LM2576HVS have their schematic inside Altium. Because the PCB will split up, the diagram is modified with suitable connectors to provide a connection between each other.

### Altium PCB design

After drawing the schematics, the PCB can be created.

#### LED driver

The schematics of the LED driver and its associated components have their PCB. This way it is possible to upgrade to more than four LED drivers or replace a defective one. The schematics are modified so that the necessary connections between the ESP32-WROVER-B and the LED driver can be made.

#### ESP32-WROVER-B

The second PCB is a merge between the ESP32 and the LM2576HVS schematic. The LM2576HVS provides the voltage for the ESP32 and is therefore chosen to be placed on the same PCB for convenience. The tracks connected to the LM2576HVS module should withstand more current. Therefore the width of associated tracks is increased.

# Results

## LED drivers

### Operation

The led drivers deliver the controlled current for each chain of LEDs. For this project, 4 LED drivers are used to control 4 different LED chains individually.

#### MagI3C

Each LED driver has its own MagI3C module. The MagI3C is the core of the LED driver and is responsible for the current controlling functionality. The module can also process PWM signals easily and thereby adjust the brightness of the LED chain. [3]

#### Determine current

The amount of current is determined by connecting a resistor to one of the pins on the magI3C. The resistance value determines the amount of current the module will provide to the LED chain. The magI3C datasheet consists of a formula to calculate the amount of current a certain resistance value will generate. [3] The PCB consists of a potentiometer and two through-hole resistor pads to solder a fixed resistor value to. One of three options can be selected using jumpers.

#### PWM

A PWM signal can be applied to the jumper tied to a pin of the magI3C module. To use the module without PWM, a constant voltage above 1.25V must be connected to the jumper. All signals below 1.25V will disable the module. [3]

#### Noise reduction.

In addition, there are 4 capacitors and 3 coils per LED driver. The capacitors and coils have noise reducing properties. A signal with less noise improves the lifetime of the LEDs and is therefore recommended.

### Schematic

Diagram, schematic

Description automatically generated

### PCB design

Graphical user interface

Description automatically generated

### Mechanical design

![A picture containing engineering drawing

Description automatically generated]()

### Finalized product

A picture containing text, electronics

Description automatically generated

## Voltage regulator

### Operation

The LM2576 step-down module and its associated components such as capacitors, inductors and resistors take power from an external power supply and converts it to 3.3V. This is used to power the esp32 module.

#### ESP32

The voltage divider connected to one of the LM2576 pins determines the voltage output. [2] The voltage divider resistor values are selected to provide the ESP32 with its recommended 3.3V. Capacitors and inductors reduce the noise on the signal and thus increasing the lifetime of the ESP32.

#### LED drivers

The voltage driving the LED drivers is not regulated by the LM2576. The led drivers are, in addition to a coil and 3 capacitors, connected to the output voltage of the external power supply. The coil and capacitors counteracts pollution to the grid caused by the use of LEDs.

### Schematic

Diagram, schematic

Description automatically generated

### PCB design

A screenshot of a video game

Description automatically generated

### Mechanical design

![Engineering drawing

Description automatically generated]()

### Finalized product

A picture containing text, electronics, circuit

Description automatically generated

## ESP32

### Operation

The ESP32 module is the brain of this project. It generates PWM signals, day/night cycles and allows for wireless control. [1]

#### User interface

The ESP32 creates a web interface. This allows for easy controlling and programming of the ESP32. [4]

#### PWM

The most important feature of the ESP32 is generating 4 individual PWM signals. These PWM signals connected to the LED drivers dim the LED chains accordingly. [1] Controlling each LED chain with an individual PWM signal allows for mixing different light spectrums and thus providing control over the total light spectrum. Because each phase of plant growth prefers a specific light spectrum, crop yield can be improved when controlling it accordingly.

#### Day/night cycles

Day and night cycles determine the on and off time of the LEDs. Through the web interface you can automate this or switch it on and off manually.

#### Programming

The ESP32's UART is available on K5 for serial communication or for programming the ESP32 in bootloader mode. The terminals DTR and RTS on K5 are connected to transistors T1 and T2 which automatically puts the ESP32 into bootloader mode. Bootloader mode can also be activated manually using button S1 and S2 and can then be programmed through K6. It can also be programmed with I²C using K7. [1]

### Schematic

Diagram, schematic

Description automatically generated

### PCB design

A screenshot of a video game

Description automatically generated

### Mechanical design

![Engineering drawing

Description automatically generated]()

### Finalized product

A picture containing text, electronics, circuit

Description automatically generated

# Discussion

## Difficulties

### LEDS

There are so many different LEDs and finding the appropriate one for a particular application is not easy. So is finding a supplier for these LEDs not easy either. Researching the different LEDs is time consuming but is the most important part of the project and therefore cannot be dismissed.

### Backorder

During the ordering process a component went temporarily out of stock. In this case the schottky diode was only available through backorder. However, the schottky diode became available through another supplier and was therefore ordered from there.

### Enabling LED driver

Testing of the LED drivers didn’t show voltage on the output. After several hours of investigation, it was noticed that the jumper connected to the PWM DIM pin of the MagI3C module was always grounded through a trace on the PCB. A connection to the ground on this pin caused the module to be switched off.

To activate the module, a voltage above 1.25V is required on the jumper. [3] The PCB is designed so that the jumper is always connected to a PWM signal. This is not a design flaw but something that was not anticipated.

## Reflection

### PCB silkscreen

The polarity was forgotten to be marked next to the input and output connectors. This required the use of a multimeter to determine the polarity.

### Programming

Programming the ESP32 is being done using the Ardiuno IDE and the associated code published by Elektor [1]. The code is no longer up to date and some of the associated libraries are no longer supported. This could be the reason why errors are occuring during compalition of the associated code.

## Conclusion

In a future project, more attention should be spent on the markings next to the components. The LED driver is completely functional and a similar designing approach will be applied in the future.

Reference list

|  |  |
| --- | --- |
| [1] | L. Lemmens, „LED-kweekbox,” Elektor, 8 9 2019. [Online]. Available: https://www.elektormagazine.nl/magazine/elektor-112/51089. [Geopend 2020]. |
| [2] | T. Instruments, „LM2576xx datasheet,” 6 1999. [Online]. Available: https://www.ti.com/lit/ds/symlink/lm2576.pdf?ts=1622049672580&ref\_url=https%253A%252F%252Fwww.google.com%252F. [Geopend 2021]. |
| [3] | W. Elektronik, „MagI3C Power Module,” 5 2016. [Online]. Available: https://www.we-online.com/catalog/en/MAGIC-LDHM-TOP263-7EP. [Geopend 2021]. |
| [4] | Espressif, „ESP32-Wrover-B Datasheet,” 1 2021. [Online]. Available: https://www.espressif.com/sites/default/files/documentation/esp32-wrover-b\_datasheet\_en.pdf. [Geopend 2021]. |
| [5] | Lumileds, „Luxeon Sunplus 35,” 2019. [Online]. Available: https://www.lumileds.com/products/horticulture-leds/luxeon-sunplus-35-line/. [Geopend 2021]. |
| [6] | W. E. Group, „YouTube,” Würth Elektronik Group, 19 3 2020. [Online]. Available: https://www.youtube.com/watch?v=2nH48m71nWI&t=732s. [Geopend 2020]. |
| [7] | W. E. Group, „YouTube,” Würth Elektronik Group, 24 9 2018. [Online]. Available: https://www.youtube.com/watch?v=OU1vD2DDwic. [Geopend 2020]. |